SOUND

*Steps to power on the sound board, speakers and sub (woofer).*

IN THIS ORDER…

1. Turn on sub woofer that sits on the stage on the back of the box. You will not hear anything as the board will not have been turned on yet.
2. Flip the POWER button on in the tech booth. This will power on the board, sub and speakers one at a time so that no pops or noise are heard.
3. On the sound board, push the small white View Scene button and on the LED Screen select MASTER \*\*\* (now the only scene on there). Click load and confirm with the arrow keys. This scene has been eq’d by a professional so please do not make ANY changes without talking to Sabrina.
4. On the stage in the rack, push the 2 soft buttons on the In Ear Monitor component.

FYI – piano and drums are now on 2 channels each (left and right).

There are now 3 DCA’s – Drums, Band (all instruments without drums: piano/bass/ac gtr/egtr/synth) and Vocals. You can now mix with only these 3 faders on the right side of the board (channels are red).

**PLEASE VIEW THE VIDEO ON DCA’S FOR MORE DETAILS.**

POWER OFF – In this order…

1. Turn off sub on stage.
2. On board LED screen choose set up button (like usual) and hit shutdown button and confirm with the arrow keys.
3. Turn off Power Switch – everything will power off in sequence to prevent pops.
4. Place cover back on board.
5. **Remove all personal effects and clean up area**.

Thank you !!!